
McMaster Spring

<http://www.mcmaster.com/#1986k48/=sy6riq>

### Type 302 Stainless Steel Compression Spring

### 1.750" Length, .156" OD, .016" Wire Diameter



Packs of 6

In stock

$4.76 per pack of 6

1986K48

3 added to your order [07/22/14](http://www.mcmaster.com/).

|  |  |
| --- | --- |
| Spring OD | 0.156" |
| Wire Diameter | 0.016" |
| Compressed Length | 0.43" |
| Maximum Load | 1.63 lbs. |
| Rate | 1.24 lbs./inch |
| Additional Specifications | Type 302 Stainless Steel—Closed Ends |
|  | 1.75" Overall Length |

Count on these springs for corrosion resistance.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Distance Plunger Displaced (mm) | Liquid Dispensed  (mL) |  |  |  |  |
| 33.52 | 0.57 |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |